Download the YOLOv8 model

Given the coordinates calculate the distance between the boxes coordinates

Fetch the output data in the form of bounding box coordinates

Feed the image data to quantized model

NNCF Post-training Quantization

Convert into OpenVINO IR model

if distance<threshold

Person violated

Person non-violated

Change the frames accordingly

Desired Output

Yes No